,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Light Source Parameter##Other##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Symmetric Medium Beam RGBW RGBW (139-1877),FLC240 CC LED - 139-1877,139-1877,"Symmetric, Medium Beam [M] - LED-24/96W - RGBW","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-1877,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-1877,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash RGBW RGBW (139-1877+139-1854),FLC240 CC LED - 139-1877+139-1854,139-1877+139-1854,Wallwash - LED-24/96W - RGBW,"RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-1877,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-1877+139-1854,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam RGBW RGBW (139-1879),FLC240 CC LED - 139-1879,139-1879,"Symmetric, Narrow Beam [E] - LED-24/96W - RGBW","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-1879,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-1879,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Narrow Beam RGBW RGBW (139-1879+139-1855),FLC240 CC LED - 139-1879+139-1855,139-1879+139-1855,"Linear Spread, Narrow Beam [E] - LED-24/96W - RGBW","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-1879,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-1879+139-1855,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam RGBW RGBW (139-1931),FLC240 CC LED - 139-1931,139-1931,"Symmetric, Wide Beam [B] - LED-24/96W - RGBW","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-1931,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-1931,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 96W RGBA (139-2140),FLC240 CC LED - 139-2140,139-2140,"Symmetric, Wide Beam [B] - LED-24/96W - RGBA","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-2140,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-2140,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 96W RGBA (139-2141),FLC240 CC LED - 139-2141,139-2141,"Symmetric, Narrow Beam [E] - LED-24/96W - RGBA","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-2141,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-2141,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Narrow Beam 96W RGBA (139-2141+139-1855),FLC240 CC LED - 139-2141+139-1855,139-2141+139-1855,"Linear Spread, Narrow Beam [E] - LED-24/96W - RGBA","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-2141,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-2141+139-1855,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 96W RGBA (139-2142),FLC240 CC LED - 139-2142,139-2142,"Symmetric, Medium Beam [M] - LED-24/96W - RGBA","RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-2142,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-2142,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 96W RGBA (139-2142+139-1854),FLC240 CC LED - 139-2142+139-1854,139-2142+139-1854,Wallwash - LED-24/96W - RGBA,"RGBW/RGBA Colour Changer. RGBW (white in 4000 K, 3000 K available on request) and RGBA (amber in 1850 K). IP66. Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Two cable glands.  Integral EC electronic converter in thermally separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. LED circuit board with WE-EF Colour Boost Technology. DMX Interface. For other control interface options to suit specific project requirements, contact WE-EF.  ",https://www.we-ef.com/#!/asia/products/family/flc240-cc-led/139-2142,WE-EF,https://www.we-ef.com/#!/asia,340,197,410,0,100,Lighting,SelfIllumination_RGB_WE-EF,z_FLC240_CC_LED : 139-2142+139-1854,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
