,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Light Source Parameter##Other##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Symmetric Medium Beam 24W 3000K (145-9556),FLD131 LED RAIL66 - 145-9556,145-9556,"Symmetric, Medium Beam [M] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9556,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9556,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Wallwash 24W 3000K (145-9556+145-9577),FLD131 LED RAIL66 - 145-9556+145-9577,145-9556+145-9577,Wallwash - LED-12/24W / 700 MA - 3000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9556,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9556+145-9577,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam 24W 3000K (145-9557),FLD131 LED RAIL66 - 145-9557,145-9557,"Symmetric, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9557,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9557,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Medium Beam 24W 4000K (145-9559),FLD131 LED RAIL66 - 145-9559,145-9559,"Symmetric, Medium Beam [M] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9559,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9559,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Wallwash 24W 4000K (145-9559+145-9577),FLD131 LED RAIL66 - 145-9559+145-9577,145-9559+145-9577,Wallwash - LED-12/24W / 700 MA - 4000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9559,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9559+145-9577,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam 24W 4000K (145-9560),FLD131 LED RAIL66 - 145-9560,145-9560,"Symmetric, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9560,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9560,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Wide Beam 24W 3000K (145-9608),FLD131 LED RAIL66 - 145-9608,145-9608,"Symmetric, Wide Beam [B] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9608,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9608,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam Sharp Cut-Off 24W 3000K (145-9609),FLD131 LED RAIL66 - 145-9609,145-9609,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9609,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9609,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Wide Beam 24W 4000K (145-9610),FLD131 LED RAIL66 - 145-9610,145-9610,"Symmetric, Wide Beam [B] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9610,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9610,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam Sharp Cut-Off 24W 4000K (145-9611),FLD131 LED RAIL66 - 145-9611,145-9611,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system. 2700 K option available on request.  ",https://www.we-ef.com/#!/aus/products/family/fld131-led-rail66/145-9611,WE-EF,https://www.we-ef.com/#!/aus,200,80,314,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLD131_LED_RAIL66 : 145-9611,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
