,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Light Source Parameter##Other##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Symmetric Wide Beam 48W 2700K (146-0984),FLC141 LED RAIL66 - 146-0984,146-0984,"Symmetric, Wide Beam [B] - LED-24/48W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0984,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0984,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Medium Beam 48W 2700K (146-0985),FLC141 LED RAIL66 - 146-0985,146-0985,"Symmetric, Medium Beam [M] - LED-24/48W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0985,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0985,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Wallwash 48W 2700K (146-0985+146-0646),FLC141 LED RAIL66 - 146-0985+146-0646,146-0985+146-0646,Wallwash - LED-24/48W / 700 MA - 2700 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0985,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0985+146-0646,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam 48W 2700K (146-0986),FLC141 LED RAIL66 - 146-0986,146-0986,"Symmetric, Very Narrow Beam [EE] - LED-24/48W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0986,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0986,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Linear Spread Very Narrow Beam 48W 2700K (146-0986+146-0439),FLC141 LED RAIL66 - 146-0986+146-0439,146-0986+146-0439,"Linear Spread, Very Narrow Beam [EE] - LED-24/48W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0986,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0986+146-0439,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam Sharp Cut-Off 48W 2700K (146-0987),FLC141 LED RAIL66 - 146-0987,146-0987,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-24/48W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0987,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0987,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Linear Spread Very Narrow Beam Sharp Cut-Off 48W 2700K (146-0987+146-0439),FLC141 LED RAIL66 - 146-0987+146-0439,146-0987+146-0439,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-24/48W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-0987,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC141_LED_RAIL66 : 146-0987+146-0439,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Medium Beam 48W 3000K (146-7058),FLC141 LED RAIL66 - 146-7058,146-7058,"Symmetric, Medium Beam [M] - LED-24/48W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7058,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7058,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Wallwash 48W 3000K (146-7058+146-0646),FLC141 LED RAIL66 - 146-7058+146-0646,146-7058+146-0646,Wallwash - LED-24/48W / 700 MA - 3000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7058,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7058+146-0646,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Medium Beam 48W 4000K (146-7059),FLC141 LED RAIL66 - 146-7059,146-7059,"Symmetric, Medium Beam [M] - LED-24/48W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7059,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7059,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Wallwash 48W 4000K (146-7059+146-0646),FLC141 LED RAIL66 - 146-7059+146-0646,146-7059+146-0646,Wallwash - LED-24/48W / 700 MA - 4000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7059,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7059+146-0646,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam Sharp Cut-Off 48W 3000K (146-7060),FLC141 LED RAIL66 - 146-7060,146-7060,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-24/48W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7060,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7060,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Linear Spread Very Narrow Beam Sharp Cut-Off 48W 3000K (146-7060+146-0439),FLC141 LED RAIL66 - 146-7060+146-0439,146-7060+146-0439,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-24/48W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7060,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7060+146-0439,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam Sharp Cut-Off 48W 4000K (146-7061),FLC141 LED RAIL66 - 146-7061,146-7061,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-24/48W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7061,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7061,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Linear Spread Very Narrow Beam Sharp Cut-Off 48W 4000K (146-7061+146-0439),FLC141 LED RAIL66 - 146-7061+146-0439,146-7061+146-0439,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-24/48W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7061,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7061+146-0439,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Wide Beam 48W 3000K (146-7070),FLC141 LED RAIL66 - 146-7070,146-7070,"Symmetric, Wide Beam [B] - LED-24/48W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7070,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7070,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Wide Beam 48W 4000K (146-7071),FLC141 LED RAIL66 - 146-7071,146-7071,"Symmetric, Wide Beam [B] - LED-24/48W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7071,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7071,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam 48W 3000K (146-7072),FLC141 LED RAIL66 - 146-7072,146-7072,"Symmetric, Very Narrow Beam [EE] - LED-24/48W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7072,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7072,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Linear Spread Very Narrow Beam 48W 3000K (146-7072+146-0439),FLC141 LED RAIL66 - 146-7072+146-0439,146-7072+146-0439,"Linear Spread, Very Narrow Beam [EE] - LED-24/48W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7072,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_3000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7072+146-0439,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Symmetric Very Narrow Beam 48W 4000K (146-7073),FLC141 LED RAIL66 - 146-7073,146-7073,"Symmetric, Very Narrow Beam [EE] - LED-24/48W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7073,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7073,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
Linear Spread Very Narrow Beam 48W 4000K (146-7073+146-0439),FLC141 LED RAIL66 - 146-7073+146-0439,146-7073+146-0439,"Linear Spread, Very Narrow Beam [EE] - LED-24/48W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Safety glass lens. Silicone CCG_R_ Controlled Compression Gasket. Luminaire is factory-sealed and does not need to be opened during installation.  Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept.  Including 0.4 m of flexible cable enclosed in a stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/asia/products/family/flc141-led-rail66/146-7073,WE-EF,https://www.we-ef.com/#!/asia,242,70,352,0,55,Lighting,SelfIllumination_4000k_WE-EF,z_FLC141_LED_RAIL66 : 146-7073+146-0439,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200813
