,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Light Source Parameter##Other##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Wallwash 12W 3000K (145-0245),FLD121 LED RAIL66 - 145-0245,145-0245,Wallwash [A20] - LED-6/12W / 700 MA - 3000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-0245,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_3000k_WE-EF,z_FLD121_LED_RAIL66 : 145-0245,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Wallwash 12W 4000K (145-0246),FLD121 LED RAIL66 - 145-0246,145-0246,Wallwash [A20] - LED-6/12W / 700 MA - 4000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-0246,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_4000k_WE-EF,z_FLD121_LED_RAIL66 : 145-0246,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Medium Beam 12W 3000K (145-9509),FLD121 LED RAIL66 - 145-9509,145-9509,"Symmetric, Medium Beam [M] - LED-6/12W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9509,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_3000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9509,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Medium Beam 12W 4000K (145-9510),FLD121 LED RAIL66 - 145-9510,145-9510,"Symmetric, Medium Beam [M] - LED-6/12W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9510,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_4000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9510,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Wide Beam 12W 3000K (145-9511),FLD121 LED RAIL66 - 145-9511,145-9511,"Symmetric, Wide Beam [B] - LED-6/12W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9511,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_3000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9511,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Wide Beam 12W 4000K (145-9512),FLD121 LED RAIL66 - 145-9512,145-9512,"Symmetric, Wide Beam [B] - LED-6/12W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9512,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_4000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9512,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Very Narrow Beam 12W 3000K (145-9513),FLD121 LED RAIL66 - 145-9513,145-9513,"Symmetric, Very Narrow Beam [EE] - LED-6/12W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9513,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_3000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9513,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Very Narrow Beam 12W 4000K (145-9514),FLD121 LED RAIL66 - 145-9514,145-9514,"Symmetric, Very Narrow Beam [EE] - LED-6/12W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9514,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_4000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9514,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Very Narrow Beam Sharp Cut-Off 12W 3000K (145-9515),FLD121 LED RAIL66 - 145-9515,145-9515,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-6/12W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9515,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_3000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9515,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Very Narrow Beam Sharp Cut-Off 12W 4000K (145-9516),FLD121 LED RAIL66 - 145-9516,145-9516,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-6/12W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Integral EC electronic converter in thermally seperated compartment. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board. Including 0,4 m of flexible cable enclosed in stainless conduit, in-line connector and mounting clamp for installation to RAIL66 mounting system.  ",https://www.we-ef.com/#!/int/products/family/fld121-led-rail66/145-9516,WE-EF,https://www.we-ef.com/#!/int,175,75,335,0,15,Lighting,SelfIllumination_4000k_WE-EF,z_FLD121_LED_RAIL66 : 145-9516,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
