,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Light Source Parameter##Other##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Symmetric Medium Beam 24W 3000K (139-1830),FLC230 LED - 139-1830,139-1830,"Symmetric, Medium Beam [M] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1830,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1830,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 24W 3000K (139-1830+139-1848),FLC230 LED - 139-1830+139-1848,139-1830+139-1848,Wallwash - LED-12/24W / 700 MA - 3000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1830,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1830+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 24W 4000K (139-1831),FLC230 LED - 139-1831,139-1831,"Symmetric, Medium Beam [M] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1831,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1831,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 24W 4000K (139-1831+139-1848),FLC230 LED - 139-1831+139-1848,139-1831+139-1848,Wallwash - LED-12/24W / 700 MA - 4000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1831,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1831+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 24W 3000K (139-1832),FLC230 LED - 139-1832,139-1832,"Symmetric, Narrow Beam [E] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1832,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1832,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 24W 4000K (139-1833),FLC230 LED - 139-1833,139-1833,"Symmetric, Narrow Beam [E] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1833,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1833,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 24W 3000K (139-1834),FLC230 LED - 139-1834,139-1834,"Symmetric, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1834,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1834,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 24W 3000K (139-1834+139-1849),FLC230 LED - 139-1834+139-1849,139-1834+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1834,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1834+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 24W 4000K (139-1835),FLC230 LED - 139-1835,139-1835,"Symmetric, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1835,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1835,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 24W 4000K (139-1835+139-1849),FLC230 LED - 139-1835+139-1849,139-1835+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1835,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1835+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 36W 3000K (139-1836),FLC230 LED - 139-1836,139-1836,"Symmetric, Medium Beam [M] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1836,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1836,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 36W 3000K (139-1836+139-1848),FLC230 LED - 139-1836+139-1848,139-1836+139-1848,Wallwash - LED-12/36W / 1050 MA - 3000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1836,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1836+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 36W 4000K (139-1837),FLC230 LED - 139-1837,139-1837,"Symmetric, Medium Beam [M] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1837,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1837,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 36W 4000K (139-1837+139-1848),FLC230 LED - 139-1837+139-1848,139-1837+139-1848,Wallwash - LED-12/36W / 1050 MA - 4000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1837,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1837+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 36W 3000K (139-1838),FLC230 LED - 139-1838,139-1838,"Symmetric, Narrow Beam [E] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1838,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1838,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 36W 4000K (139-1839),FLC230 LED - 139-1839,139-1839,"Symmetric, Narrow Beam [E] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1839,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1839,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 36W 3000K (139-1840),FLC230 LED - 139-1840,139-1840,"Symmetric, Very Narrow Beam [EE] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1840,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1840,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 36W 3000K (139-1840+139-1849),FLC230 LED - 139-1840+139-1849,139-1840+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1840,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1840+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 36W 4000K (139-1841),FLC230 LED - 139-1841,139-1841,"Symmetric, Very Narrow Beam [EE] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1841,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1841,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 36W 4000K (139-1841+139-1849),FLC230 LED - 139-1841+139-1849,139-1841+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1841,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1841+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 52W 3000K (139-1842),FLC230 LED - 139-1842,139-1842,"Symmetric, Medium Beam [M] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1842,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1842,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 52W 3000K (139-1842+139-1848),FLC230 LED - 139-1842+139-1848,139-1842+139-1848,Wallwash - LED-12/52W / 1400 MA - 3000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1842,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1842+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 52W 4000K (139-1843),FLC230 LED - 139-1843,139-1843,"Symmetric, Medium Beam [M] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1843,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1843,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 52W 4000K (139-1843+139-1848),FLC230 LED - 139-1843+139-1848,139-1843+139-1848,Wallwash - LED-12/52W / 1400 MA - 4000 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1843,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1843+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 52W 3000K (139-1844),FLC230 LED - 139-1844,139-1844,"Symmetric, Narrow Beam [E] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1844,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1844,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 52W 4000K (139-1845),FLC230 LED - 139-1845,139-1845,"Symmetric, Narrow Beam [E] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1845,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1845,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 52W 3000K (139-1846),FLC230 LED - 139-1846,139-1846,"Symmetric, Very Narrow Beam [EE] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1846,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1846,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 52W 3000K (139-1846+139-1849),FLC230 LED - 139-1846+139-1849,139-1846+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1846,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1846+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 52W 4000K (139-1847),FLC230 LED - 139-1847,139-1847,"Symmetric, Very Narrow Beam [EE] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1847,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1847,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 52W 4000K (139-1847+139-1849),FLC230 LED - 139-1847+139-1849,139-1847+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1847,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1847+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 24W 3000K (139-1901),FLC230 LED - 139-1901,139-1901,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1901,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1901,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 24W 3000K (139-1901+139-1849),FLC230 LED - 139-1901+139-1849,139-1901+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1901,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1901+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 24W 4000K (139-1902),FLC230 LED - 139-1902,139-1902,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1902,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1902,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 24W 4000K (139-1902+139-1849),FLC230 LED - 139-1902+139-1849,139-1902+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1902,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1902+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 36W 3000K (139-1903),FLC230 LED - 139-1903,139-1903,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1903,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1903,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 36W 3000K (139-1903+139-1849),FLC230 LED - 139-1903+139-1849,139-1903+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1903,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1903+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 36W 4000K (139-1904),FLC230 LED - 139-1904,139-1904,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1904,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1904,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 36W 4000K (139-1904+139-1849),FLC230 LED - 139-1904+139-1849,139-1904+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1904,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1904+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 52W 3000K (139-1905),FLC230 LED - 139-1905,139-1905,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1905,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1905,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 52W 3000K (139-1905+139-1849),FLC230 LED - 139-1905+139-1849,139-1905+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1905,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1905+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 52W 4000K (139-1906),FLC230 LED - 139-1906,139-1906,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1906,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1906,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 52W 4000K (139-1906+139-1849),FLC230 LED - 139-1906+139-1849,139-1906+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1906,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1906+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 24W 3000K (139-1907),FLC230 LED - 139-1907,139-1907,"Symmetric, Wide Beam [B] - LED-12/24W / 700 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1907,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1907,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 24W 4000K (139-1908),FLC230 LED - 139-1908,139-1908,"Symmetric, Wide Beam [B] - LED-12/24W / 700 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1908,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1908,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 36W 3000K (139-1909),FLC230 LED - 139-1909,139-1909,"Symmetric, Wide Beam [B] - LED-12/36W / 1050 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1909,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1909,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 36W 4000K (139-1910),FLC230 LED - 139-1910,139-1910,"Symmetric, Wide Beam [B] - LED-12/36W / 1050 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1910,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,43,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1910,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 52W 3000K (139-1911),FLC230 LED - 139-1911,139-1911,"Symmetric, Wide Beam [B] - LED-12/52W / 1400 MA - 3000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1911,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_3000k_WE-EF,z_FLC230_LED : 139-1911,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 52W 4000K (139-1912),FLC230 LED - 139-1912,139-1912,"Symmetric, Wide Beam [B] - LED-12/52W / 1400 MA - 4000 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-1912,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_4000k_WE-EF,z_FLC230_LED : 139-1912,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 36W 2700K (139-2077),FLC230 LED - 139-2077,139-2077,"Symmetric, Very Narrow Beam [EE] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2077,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2077,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 36W 2700K (139-2077+139-1849),FLC230 LED - 139-2077+139-1849,139-2077+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2077,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2077+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 36W 2700K (139-2079),FLC230 LED - 139-2079,139-2079,"Symmetric, Narrow Beam [E] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2079,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2079,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 52W 2700K (139-2108),FLC230 LED - 139-2108,139-2108,"Symmetric, Medium Beam [M] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2108,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2108,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 52W 2700K (139-2108+139-1848),FLC230 LED - 139-2108+139-1848,139-2108+139-1848,Wallwash - LED-12/52W / 1400 MA - 2700 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2108,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2108+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 24W 2700K (139-2151),FLC230 LED - 139-2151,139-2151,"Symmetric, Medium Beam [M] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2151,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2151,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 24W 2700K (139-2151+139-1848),FLC230 LED - 139-2151+139-1848,139-2151+139-1848,Wallwash - LED-12/24W / 700 MA - 2700 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2151,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2151+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 52W 2700K (139-2191),FLC230 LED - 139-2191,139-2191,"Symmetric, Very Narrow Beam [EE] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2191,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2191,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 52W 2700K (139-2191+139-1849),FLC230 LED - 139-2191+139-1849,139-2191+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2191,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2191+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 52W 2700K (139-2214),FLC230 LED - 139-2214,139-2214,"Symmetric, Narrow Beam [E] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2214,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2214,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 52W 2700K (139-2226),FLC230 LED - 139-2226,139-2226,"Symmetric, Wide Beam [B] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2226,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2226,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 36W 2700K (139-2239),FLC230 LED - 139-2239,139-2239,"Symmetric, Wide Beam [B] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2239,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2239,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Medium Beam 36W 2700K (139-2240),FLC230 LED - 139-2240,139-2240,"Symmetric, Medium Beam [M] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2240,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2240,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Wallwash 36W 2700K (139-2240+139-1848),FLC230 LED - 139-2240+139-1848,139-2240+139-1848,Wallwash - LED-12/36W / 1050 MA - 2700 K,"IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2240,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2240+139-1848,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Wide Beam 24W 2700K (139-2241),FLC230 LED - 139-2241,139-2241,"Symmetric, Wide Beam [B] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2241,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,26,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2241,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Narrow Beam 24W 2700K (139-2242),FLC230 LED - 139-2242,139-2242,"Symmetric, Narrow Beam [E] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2242,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2242,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam 24W 2700K (139-2263),FLC230 LED - 139-2263,139-2263,"Symmetric, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2263,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2263,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam 24W 2700K (139-2263+139-1849),FLC230 LED - 139-2263+139-1849,139-2263+139-1849,"Linear Spread, Very Narrow Beam [EE] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2263,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,55,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2263+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 24W 2700K (139-2264),FLC230 LED - 139-2264,139-2264,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2264,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2264,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 24W 2700K (139-2264+139-1849),FLC230 LED - 139-2264+139-1849,139-2264+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/24W / 700 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2264,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,28,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2264+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 36W 2700K (139-2271),FLC230 LED - 139-2271,139-2271,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2271,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2271,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 36W 2700K (139-2271+139-1849),FLC230 LED - 139-2271+139-1849,139-2271+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/36W / 1050 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2271,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,42,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2271+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Very Narrow Beam Sharp Cut-Off 52W 2700K (139-2279),FLC230 LED - 139-2279,139-2279,"Symmetric, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2279,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2279,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Linear Spread Very Narrow Beam Sharp Cut-Off 52W 2700K (139-2279+139-1849),FLC230 LED - 139-2279+139-1849,139-2279+139-1849,"Linear Spread, Very Narrow Beam, 'Sharp Cut-Off' [EES] - LED-12/52W / 1400 MA - 2700 K","IP66, Class I. IK07. Marine-grade, die-cast aluminium alloy. 5CE superior corrosion protection including PCS hardware. Silicone CCG_R_ Controlled Compression Gasket. Safety glass lens. Two cable glands for improved wiring flexibility. Integral EC electronic converter, thermally separated. CAD-optimised optics for superior illumination and glare control. OLC_R_ One LED Concept. Factory installed LED circuit board.  1-10V, DALI Interface or Eco Step Dim_R_ on request. Maximum one internal optical accessory possible.  ",https://www.we-ef.com/#!/aus/products/family/flc230-led/139-2279,WE-EF,https://www.we-ef.com/#!/aus,260,160,325,0,56,Lighting,SelfIllumination_2700k_WE-EF,z_FLC230_LED : 139-2279+139-1849,230,0.9,Pr_70_70_48_82,Spotlights,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
