,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,Light Source Parameter##Other##,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Symmetric Linear Wide Beam 50W 3000K (187-0027),VLR150 - 187-0027,187-0027,"Symmetric Linear, Wide Beam [LB] - LED-80/50W / 225 MA - 3000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0027,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0027,55,Lighting,SelfIllumination_3000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Medium Beam 50W 3000K (187-0028),VLR150 - 187-0028,187-0028,"Symmetric Linear, Medium Beam [LM] - LED-80/50W / 225 MA - 3000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0028,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0028,55,Lighting,SelfIllumination_3000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Narrow Beam 50W 3000K (187-0029),VLR150 - 187-0029,187-0029,"Symmetric Linear, Narrow Beam [LE] - LED-80/50W / 225 MA - 3000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0029,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0029,55,Lighting,SelfIllumination_3000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Very Narrow Beam 50W 3000K (187-0030),VLR150 - 187-0030,187-0030,"Symmetric Linear, Very Narrow Beam [LEE] - LED-80/50W / 225 MA - 3000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0030,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0030,55,Lighting,SelfIllumination_3000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Wide Beam 50W 4000K (187-0047),VLR150 - 187-0047,187-0047,"Symmetric Linear, Wide Beam [LB] - LED-80/50W / 225 MA - 4000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0047,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0047,55,Lighting,SelfIllumination_4000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Medium Beam 50W 4000K (187-0048),VLR150 - 187-0048,187-0048,"Symmetric Linear, Medium Beam [LM] - LED-80/50W / 225 MA - 4000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0048,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0048,55,Lighting,SelfIllumination_4000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Narrow Beam 50W 4000K (187-0049),VLR150 - 187-0049,187-0049,"Symmetric Linear, Narrow Beam [LE] - LED-80/50W / 225 MA - 4000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0049,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0049,55,Lighting,SelfIllumination_4000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Very Narrow Beam 50W 4000K (187-0050),VLR150 - 187-0050,187-0050,"Symmetric Linear, Very Narrow Beam [LEE] - LED-80/50W / 225 MA - 4000 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0050,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0050,55,Lighting,SelfIllumination_4000k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Wide Beam 50W 2700K (187-0545),VLR150 - 187-0545,187-0545,"Symmetric Linear, Wide Beam [LB] - LED-80/50W / 225 MA - 2700 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0545,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0545,55,Lighting,SelfIllumination_2700k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Narrow Beam 50W 2700K (187-0546),VLR150 - 187-0546,187-0546,"Symmetric Linear, Narrow Beam [LE] - LED-80/50W / 225 MA - 2700 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0546,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0546,55,Lighting,SelfIllumination_2700k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Very Narrow Beam 50W 2700K (187-0547),VLR150 - 187-0547,187-0547,"Symmetric Linear, Very Narrow Beam [LEE] - LED-80/50W / 225 MA - 2700 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0547,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0547,55,Lighting,SelfIllumination_2700k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
Symmetric Linear Medium Beam 50W 2700K (187-0548),VLR150 - 187-0548,187-0548,"Symmetric Linear, Medium Beam [LM] - LED-80/50W / 225 MA - 2700 K","IP66, Class I. IK09. Marine-grade, all-aluminium construction. 5CE superior corrosion protection including PCS hardware. PMMA lens. Silicone rubber gaskets. 1.2 m of flexible PVC-free cable. Luminaire is factory-sealed and does not need to be opened during installation. Integral EC electronic converter in thermally-separated compartment. Advanced thermal management protects LEDs while optimising lumens output. Removable LED boards for upgrading.DALI interface.  ",https://www.we-ef.com/#!/aus/products/family/rmt320-one-sided/187-0548,WE-EF,https://www.we-ef.com/#!/asia,1528,132,58,2000,z_VLR150 : 187-0548,55,Lighting,SelfIllumination_2700k_WE-EF,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200804
