,Model##OTHER##,ManufacturerSpecCode##OTHER##,Type Comments##OTHER##,Description##OTHER##,ManufacturerURLProductSpecific##OTHER##,Manufacturer##OTHER##,URL##OTHER##,ManufacturerOverallWidth##LENGTH##MILLIMETERS,ManufacturerOverallDepth##LENGTH##MILLIMETERS,ManufacturerOverallHeight##LENGTH##MILLIMETERS,ManufacturerHeightFromFFL##LENGTH##MILLIMETERS,Tilt Angle##ANGLE##DECIMAL DEGREES,TotalWattage##ELECTRICAL_WATTAGE##WATTS,Load Classification##OTHER##,Self Illuminating Material##OTHER##,Light Source Parameter##Other##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Uniclass2015Code##OTHER##,Uniclass2015Title##OTHER##,Uniclass2015Version##OTHER##,IfcExportAs##OTHER##,IfcExportType##OTHER##,CreatedBy##OTHER##,CreatedByURL##OTHER##,ModifiedIssue##Other##
Symmetric Linear Wide Beam 50W 3000K (187-0027),VLR150 - 187-0027,187-0027,"Symmetric Linear, Wide Beam [LB] - LED-80/50W / 225 MA - 3000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0027,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_3000k_WE-EF,z_VLR150 : 187-0027,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Medium Beam 50W 3000K (187-0028),VLR150 - 187-0028,187-0028,"Symmetric Linear, Medium Beam [LM] - LED-80/50W / 225 MA - 3000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0028,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_3000k_WE-EF,z_VLR150 : 187-0028,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Narrow Beam 50W 3000K (187-0029),VLR150 - 187-0029,187-0029,"Symmetric Linear, Narrow Beam [LE] - LED-80/50W / 225 MA - 3000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0029,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_3000k_WE-EF,z_VLR150 : 187-0029,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Very Narrow Beam 50W 3000K (187-0030),VLR150 - 187-0030,187-0030,"Symmetric Linear, Very Narrow Beam [LEE] - LED-80/50W / 225 MA - 3000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0030,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_3000k_WE-EF,z_VLR150 : 187-0030,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Wide Beam 50W 4000K (187-0047),VLR150 - 187-0047,187-0047,"Symmetric Linear, Wide Beam [LB] - LED-80/50W / 225 MA - 4000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0047,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_4000k_WE-EF,z_VLR150 : 187-0047,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Medium Beam 50W 4000K (187-0048),VLR150 - 187-0048,187-0048,"Symmetric Linear, Medium Beam [LM] - LED-80/50W / 225 MA - 4000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0048,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_4000k_WE-EF,z_VLR150 : 187-0048,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Narrow Beam 50W 4000K (187-0049),VLR150 - 187-0049,187-0049,"Symmetric Linear, Narrow Beam [LE] - LED-80/50W / 225 MA - 4000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0049,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_4000k_WE-EF,z_VLR150 : 187-0049,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Very Narrow Beam 50W 4000K (187-0050),VLR150 - 187-0050,187-0050,"Symmetric Linear, Very Narrow Beam [LEE] - LED-80/50W / 225 MA - 4000 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0050,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_4000k_WE-EF,z_VLR150 : 187-0050,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Wide Beam 50W 2700K (187-0545),VLR150 - 187-0545,187-0545,"Symmetric Linear, Wide Beam [LB] - LED-80/50W / 225 MA - 2700 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0545,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_2700k_WE-EF,z_VLR150 : 187-0545,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Narrow Beam 50W 2700K (187-0546),VLR150 - 187-0546,187-0546,"Symmetric Linear, Narrow Beam [LE] - LED-80/50W / 225 MA - 2700 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0546,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_2700k_WE-EF,z_VLR150 : 187-0546,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Very Narrow Beam 50W 2700K (187-0547),VLR150 - 187-0547,187-0547,"Symmetric Linear, Very Narrow Beam [LEE] - LED-80/50W / 225 MA - 2700 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0547,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_2700k_WE-EF,z_VLR150 : 187-0547,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
Symmetric Linear Medium Beam 50W 2700K (187-0548),VLR150 - 187-0548,187-0548,"Symmetric Linear, Medium Beam [LM] - LED-80/50W / 225 MA - 2700 K","IP67, Class I. IK09. Marine-grade, all aluminium construction. 5CE superior corrosion protection including PCS hardware. Silicone rubber gasket. PMMA main lens. Linear PMMA LED lens. 1.2 m connecting cable, UV stabilized, PVC free. Luminaire is factory sealed and does not need to be opened during installation and can be tilted up to 180. Integral LED driver with DALI interface.  Separate LED driver on request.  ",https://www.we-ef.com/#!/int/products/family/vlr150/187-0548,WE-EF,https://www.we-ef.com/#!/int,1528,132,58,2000,90,55,Lighting,SelfIllumination_2700k_WE-EF,z_VLR150 : 187-0548,230,0.9,Pr_70_70_48_85,Surface luminaires,Products v1.18,IfcLightFixtureType,NOTDEFINED,IGS BIM Solutions,https://igsgroup.com.au,20200902
